Next Page | Previous Page | Index

### 58"-long x 98 1/2"-wide Landing Module

(for 42" modules)
(use 92 1/2" wide module if using 39" ramping modules)
Used for level landings in l80-degree switchback ramps and sometimes at doorway

Components:

    7    2x6 by 55" Joists (Order four 2x6x10 and cut seven joists)
    2    2x6 by 98" End Pieces (Order two 2x6x10 and cut two endpieces)
    10   5/4x6 by 98" Decking (Order ten 5/4x6 by 10 and cut ten pieces)
    140  2 1/2" Deck Screws (10 per decking plank)
    28   2 1/2" Deck Screws (to attach end pieces to joists)
    14   2x6 Joist Hangers
    112  Joist Hanger Nails

Construction Notes:

1. Cut joists and end pieces to length and assemble on flat surface. Space joists 16" apart on center.
2. Screw end pieces to the ends of joists with 3" screws.
3. Insure landing is square and nail on joist hangers.
4. Bend outside flange of four corner joist hangers flat against end pieces of landing.
5. Decking may be attached at this point or after landing frame is placed in a ramp. Decking adds significant weight to landing. If decking added, you will need to remove decking end pieces when assembling ramp.
6. 3/8" holes to allow connection to ramp modules will be drilled at time of ramp construction.

Next Page | Previous Page | Index