Next Page | Previous Page | Index

### 180 Degree Ramp Continued

- Attach string line from top of level landing to point where ramp will end.

- Bolt Module #4 to landing with 3/8"x 4" carriage bolts. Match module slope to string.

- Attach cross support for Module #4 as shown in detail 2.

- Cross supports for the junction of Modules #4 and #5 will be attached to the 4x4 at the junction of Modules #2 and #3.

#### Note: The same options for transition to the ground are used for this design.
Guardrail/handrail options are also the same except the inside guardrail on the lower portion of the ramp will be attached to the center 4x4's.
Between modules 3 & 4 some 2x2x30" spindles will need to be screwed in place from inside the ramp.

Next Page | Previous Page | Index