Next Page | Previous Page | Index

### Choosing the width of your ramp

Proper width of the ramp is important for the person using the ramp. A minimum of 36'' of clearance is needed and sometimes wider widths are advisable. The ramp modules can be made to the width that best meet the users needs. 39" and 42" wide modules have been described. If a wider ramp is desired, such as 48" wide, you need to adjust the materials ordered
Please refer to page 34 for more guardrail/handrail information!

Next Page | Previous Page | Index