Next Page | Previous Page | Index

### Right Angle Turn Transition to Ground

- Attach string line from top of level landing to point where ramp will end and attach Module #4 in the same manner as described for the top level landing.

#### NOTE: The same options for transition to the ground are used for this design.

Guardrail/handrail options are also the same except an additional 4x4 post is used at the inside corner of the landing so that guardrail can be attached at the corner of the landing.

4x4 posts are positioned so that guardrails are above outside 1 1/2" perimeter of landings and slope.
3" screws are used to attach rail to posts, always inserting screw through rail and then into 4x4

Next Page | Previous Page | Index