Next Page | Previous Page | Index

### 180 DEGREE RAMP

To build a ramp with a 180-degree turn, complete the first section of the ramp as described in previous pages (the lengths of each section do not need to be equal, ex: a 19'4" top section and a 14'6" lower section could be used). Use a 58'x98 1/2" platform and support with 98 1/2" cross supports.

- When attaching cross support for lower end of Module #3, cut 2x6 at 60-degree angle, Attach cross support to 4x4's with screws temporarily.

- Attach 98 1/2" cross support to 4x4's at end of Module #3. Insure that this cross support is level.

- Drill three 3/8" holes in 58"x98 1/2" landing to match holes in end of Module #3. The end of the level landing will be at the outside edge of the 4x4 so be sure to adjust measurements for hole alignment.

- Attach 58"x 98 1/2" platform to module 3 and support other end with jacks. Level platform and measure for 4x4's. Place 4x4's on side B as in diagram and attach cross support.

- Attach cross support to side A.

- Put 4x4 for Module #4 in place and attach with deck screws.

Next Page | Previous Page | Index