Next Page | Previous Page | Index

### 58"-long x 60"-wide Landing Module

Used for level landings in right-angle ramps and sometimes at doorway.

Components:

    5    2x6 by 55" Joists (Order three 2x6x10 and cut five joists)
    2    2x6 by 60" End Pieces (Order one 2x6x10 and cut two end pieces)
    10   5/4x6 by 60" Decking (Order five 5/4x6 by 10 and cut ten pieces)
    100  2 1/2" Deck Screws (10 per decking plank)
    20   2 1/2" Deck Screws (to attach end pieces to joists)
    10   2x6 Joist Hangers
    80   Joist Hanger Nails

Construction Notes:

1. Cut joists and end pieces to length and assemble on flat surface. Space joists 15" apart on center.
2. Screw end pieces to the ends of joists with 3" screws.
3. Insure landing is square and nail on joist hangers.
4. Bend outside flange of four corner joist hangers flat against end pieces of landing.
5. Decking may be attached at this point or after landing frame is placed in a ramp. Decking adds significant weight to landing. If decking added, you will need to remove decking end pieces when assembling ramp.
6. 3/8" holes to allow connection to ramp modules will be drilled at time of ramp construction.

Next Page | Previous Page | Index